{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Données"],"not_rendered":{"charts":0,"images":1,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Données","index":0,"n_rows":483,"n_cols":5,"rows_kept":483,"cut":false,"hidden":false,"merged":[]}
["Catégorie","Sous-catégorie","Désignation",null,{"$f":"SUBTOTAL(3,C:C)-1","v":482}]
["Barrette",null,"Barrette 1x 4 pts Mâle droite étamé  CNH 55"]
["Barrette",null,"Barrette 2x 5 pts Mâle droit doré  CNH 157"]
["Barrette",null,"Barrette 2x 6 pts Mâle droit doré  CNH 263"]
["Bouton",null,"Bouton TRAD PHAP3305A  PI 85"]
["Bouton",null,"Bouton TRAD TP33 Noir 5mm Apem  PI 51A"]
["Circuit","Intégré","Circuit intégré CMS 74HCT125 SO14  SP 227 Texas Inst"]
["Circuit","Intégré","Circuit intégré CMS AM 29F040 B-120 JC PLCC32 AMD Atmel"]
["Circuit","Intégré","Circuit intégré CMS IDT71V125S15Y SOJ32 Alliance"]
["Circuit","Intégré","Circuit intégré CMS IRF 7104 SO8 SP 94 International Rectifier"]
["Circuit","Intégré","Circuit intégré CMS MAX 6120 ESA Maxim"]
["Circuit","Intégré","Circuit intégré CMS MAX 6315 US26D4-T  µProc TO253-4  SJS 202  "]
["Circuit","Intégré","Circuit intégré CMS TLC 2274 CD SO14 SP 177 Texas Inst"]
["Circuit","Logique","Circuit logique CMS 74V1G04 STR inverseur SOT23-5  SJS 145"]
["Circuit","Logique","Circuit logique CMS 74V1G86 STR porte OU excl SOT23-5  SJS 76  "]
["Circuit","Logique","Circuit logique CMS NC 7S04M5X Inverseur SOT23-5  SJS 145  "]
["Circuit","Logique","Circuit logique CMS NC 7S14M5X Inverseur SOT23-5  SJS 196"]
["Condensateur","Céramique","Condensateur céramique TRAD 100pF 100V axial 5.08"]
["Condensateur","Chimique","Condensateur chimique TRAD 1µF 63V rad 2.54  PHC 34"]
["Condensateur","Chimique","Condensateur chimique TRAD 100µF 16V 5.08  PHP 47"]
["Condensateur","Chimique","Condensateur chimique TRAD 22µF 35V rad 5.08"]
["Condensateur","Chimique","Condensateur chimique TRAD 4.7µF 100V rad 2.54  PHP 54"]
["Condensateur","CMS","Condensateur CMS 0402  100pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0402  10nF 25V 10% X7R MCH152CN103KK"]
["Condensateur","CMS","Condensateur CMS 0402  120pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0402  330pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0402  33pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0402  390pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0402  39pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0402  680pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0402  820pF 50V / 63V 1%"]
["Condensateur","CMS","Condensateur CMS 0603  1.5nF 50V / 63V 10%  SHF 53"]
["Condensateur","CMS","Condensateur CMS 0603  10pF 50V 10% AVX 06035A100CA"]
["Condensateur","CMS","Condensateur CMS 0603  3.9nF 50V / 63V 10%  SHF 62"]
["Condensateur","CMS","Condensateur CMS 0603  560pF 50V 5%  SHF  55"]
["Condensateur","CMS","Condensateur CMS 1210  100nF 50V 10% X7R VJ1210Y104KXAT"]
["Condensateur","Electrolytique","Condensateur électrolytique Alu CMS 10µF 16V (d 4 h 5.5) EMV-160ADA100MD55N ou G"]
["Condensateur","Electrolytique","Condensateur électrolytique Alu CMS 1000µF 6V3 20%  SHE 14"]
["Condensateur","Electrolytique","Condensateur électrolytique Alu CMS 2.2µF 50V 20% (d 4 h 5.5)  SHE 5  "]
["Condensateur","Electrolytique","Condensateur électrolytique Alu CMS 4.7µF 35V 20% (d 4 h 5.3)"]
["Condensateur","Tantale","Condensateur tantale CMS 1206  2.2µF 16V 10% Boîtier A TCSCS1C225KAAR"]
["Condensateur","Tantale","Condensateur tantale CMS 2.2µF 10V 20%  SHD 64"]
["Condensateur","Tantale","Condensateur tantale CMS 4.7µF 16V 10% Boîtier B 293D475X9016B2T"]
["Condensateur",null,"Connecteur B4B PHKS 4 pts Mâle droit JST  CNH 252"]
["Condensateur",null,"Connecteur PDS 03 /5.08 à deux étages"]
["Diode","CMS","Diode CMS BAS28 double SOT23  SJS 143"]
["Diode","CMS","Diode CMS BAV70W double SOT23  SJS 130"]
["Diode","CMS","Diode CMS BAV99W double SOT23  SJS 131  "]
["Diode","CMS","Diode CMS BB148 SOD323  SJD 45"]
["Diode","CMS","Diode CMS BYD37M 1KV 1.5A SOD87  SJD 33"]
["Diode","CMS","Diode CMS DL4007  1KV 1A Melf  SJD 54"]
["Diode","CMS","Diode CMS HSMP-3820  RF SOT-23"]
["Diode","CMS","Diode CMS HSMP-3820-TR1 RF rapide SOT23"]
["Diode","CMS","Diode CMS MMBD4148 ultra rapide SOT-23"]
["Diode","CMS","Diode CMS SMBYW04-200  200V 4A  SMC  SJD 60  "]
["Diode","CMS","Diode CMS SMCJ68CA ou SM15T68CA  1.5KW 68V SMC SJD 96  "]
["Diode","CMS","Diode CMS TZMC16-GS08 16V SOD-80  SJD 7"]
["Diode","CMS","Diode CMS TZMC6V2-GS08 6,2V SOD-80  SJD 17"]
["Diode","Schottky","Diode Schottky CMS 10MQ060N TR  60V 2.1A   SJD 74  "]
["Diode","Schottky","Diode Schottky CMS BAR43SFILM SOT23  SJS 119"]
["Diode","Schottky","Diode Schottky CMS BAS70 -04 FILM  SOT23  SJS 106"]
["Diode","Schottky","Diode Schottky CMS BAS85 -07   SJD 5  "]
["Diode","Schottky","Diode Schottky CMS BAT54A LT1 SOT23  SJS 150"]
["Diode","Schottky","Diode Schottky CMS FMKA140 1A 40V DO-214"]
["Diode","Schottky","Diode Schottky CMS MBRS1100T3G 1A 100V SMB"]
["Diode","Schottky","Diode Schottky CMS MBRS130LT3 1A 30V SMB  SJD 46"]
["Diode","Schottky","Diode Schottky CMS STPS 2L25 U  2A 25V SMB  SJD 44"]
["Diode","Schottky","Diode Schottky CMS ZHCS750TA  40V IF=750mA IR=100uA SOT23  SJS 77"]
["Diode","Schottky","Diode Schottky TRAD BZX 55C 12V  PLB 19"]
["Diode","TRAD","Diode TRAD 1N4004  DO41"]
["Diode","TRAD","Diode TRAD 1N4933  PLD 3"]
["Diode","TRAD","Diode TRAD 1N914  PLD 42"]
["Diode","TRAD","Diode TRAD BAT41 DO35"]
["Diode","TRAD","Diode TRAD PH-13M  PLD 65"]
["Diode","TRAD","Diode TRAD SB130  PLD 66"]
["Diode","Transil","Diode Transil CMS SM6T12A  600W 12V SMB  SJD 90  "]
["Diode","Transil","Diode Transil CMS SM6T15CA  600W 15V SMB SJD 75  "]
["Diode","Transil","Diode Transil CMS SM6T33A  600W 33V SMB  SJD 32 / SJD 61  "]
["Diode","Zener","Diode Zener CMS BZV55-C27  27V 500mW SOD80   SJD 16"]
["Diode","Zener","Diode Zener CMS BZV55-C6V8  6.8V SJD 10"]
["Diode","Zener","Diode Zener CMS BZX284-C5V6  5.6V  SJD 41"]
["Diode","Zener","Diode Zener CMS BZX84-C12 LT1G SOT23  SJS 52  "]
["Diode","Zener","Diode Zener CMS MMSZ10T1  10V 500mW SOD-123  SJD 58"]
["Diode","Zener","Diode Zener CMS MMSZ15T1  15V 500mW SOD-123  SJD 59/SJS 69 "]
["Diode","Zener","Diode Zener CMS MMSZ5223BT1  2.7V 500mW SOD-123  SJD 77  "]
["Diode","Zener","Diode Zener CMS MMSZ5230BT1  4.7V 500mW  SJD 64/SJS 66"]
["Diode","Zener","Diode Zener CMS MMSZ5237BT1  8.2V 500mW  SJS 134  "]
["Diode","Zener","Diode Zener CMS MMSZ5245BT1  15V 500mW  SJS 133"]
["Diode","Zener","Diode Zener CMS MMSZ5249BT1  19V 500mW  SJS 132 "]
["Diode","Zener","Diode Zener CMS MMSZ5V6T1  5.6V SOD-123  SJD 112  "]
["Diode","Zener","Diode Zener CMS MMSZ6V8T1  6.8V SOD-123  SJD 73"]
["Diode","Zener","Diode Zener TRAD BZX 79 3.9V Boitier DO-35"]
["Diode","Zener","Diode Zener TRAD BZX 85C 33V"]
["Diode","Zener","Diode Zener TRAD BZX 85C 6.2V 1.3V 5%"]
["Ferrite",null,"Ferrite CMS 0603 BLM11B252SDPT  2.5 KOhm 25% 100MHz 50mA"]
["Ferrite",null,"Ferrite CMS 0805 BLM21P221SGPT  220 Ohm 2A  PNS 160  "]
["Ferrite",null,"Ferrite CMS 1206 BLM31A260SPTM00-03  26 Ohm 100MHz 500mA  PNS 107"]
["Filtre","CMS","Filtre CMS 1206  100 pF 100V NP0 EMI"]
["Filtre","TRAD","Filtre EMI TRAD ZJKD51R5 15 TDK  PNS 28"]
["Fusible",null,"Fusible CMS 1206 NANO SMDM050-02  PFP 74"]
["Led","CMS","Led CMS 1206 HSMG-H690 verte"]
["Led","CMS","Led CMS 1206 LTST-C230GKT verte 565nm 6mcd  SJL 2"]
["Led","CMS","Led CMS 1210 vert / jaune HSMF-C156  572/586nm Agilent  SJL 31  "]
["Led","CMS","Led CMS LST 676-R1S1 rouge 633nm 2-PLCC  Osram"]
["Led","CMS","Led CMS LYM676-P2Q2 jaune 591nm 2-Pin SMT T/R  SJL 27  "]
["Led","TRAD","Led TRAD Emetteurs infrarouge IR Emitter 17 Degrees"]
["Led","TRAD","Led TRAD HSDL-4230  PLL 86"]
["Led","TRAD","Led TRAD Rouge diamètre 3mm"]
["Quartz","CMS","Quartz CMS  14.7456 MHz 014745LFDD5 ou JXE75/1  PQ 82 / PQ 106  "]
["Quartz","CMS","Quartz CMS  6 MHz PBRC6.00MR50X000"]
["Quartz","TRAD","Quartz TRAD 16 MHz  PQ 54"]
["Régulateur","CMS","Régulateur CMS LK112M32TR LDO 150MA 3.2V SOT23-5  SJS 201  "]
["Régulateur","CMS","Régulateur CMS LM 1117 MP -2.5  2.5V SJS 193"]
["Régulateur","CMS","Régulateur CMS TPS 76316 DBVR LDO Lin Fix Pos 1.6V 0.15A SOT23-5  SJS 227"]
["Régulateur","TRAD","Régulateur TRAD KA337TU 3TO-2201.0A"]
["Réseau résistif",null,"Réseau résistif CMS 1206  BCN16 4A 331J7 LF 4x 330 Ohm  SGR 36"]
["Réseau résistif",null,"Réseau résistif CMS 1206  BCN16 4A 473J7 LF 4x 47 KOhm  SGR 37"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAT16-151J4  4x 150 Ohm  SGR 29"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAT16-220J4  4x 22 Ohm  SGR 35"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAT16-222J4  4x 2.2 KOhm  SGR 20"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAT16-472J4  4x 4.7 KOhm  SGR 19"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAY16-101J4  4x 100 Ohm  SGR 40"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAY16-104J4  4x 100 KOhm  SGR 12"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAY16-220J4  4x 22 Ohm  SGR 16"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAY16-330J4  4x 33 Ohm  SGR 3"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAY16-331J4  4x 330 Ohm  SGR 14"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CAY16-470J4  4x 47 Ohm  SGR 17"]
["Réseau résistif",null,"Réseau résistif CMS 1206  CN1J4-TD J   4x 1 KOhm  5%  SGR 7"]
["Réseau résistif",null,"Réseau résistif CMS 1206  MNR14 EOAB J221 4x 220 Ohm  5%  SGR 11"]
["Réseau résistif",null,"Réseau résistif CMS 1206  MNR14 EOAB J472 4x 4.7 KOhm  5%  SGR 10"]
["Résistance","Carbone","Résistance carbone TRAD 10 MOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 130 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 180 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 22 Ohm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 220 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 220 Ohm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 27 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 3.3 MOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 39 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 4.7 MOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 470 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 5.1 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 560 Ohm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 680 Ohm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 8.2 MOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 91 KOhm 5% 1/4W"]
["Résistance","Carbone","Résistance carbone TRAD 910 Ohm 5% 1/4W"]
["Résistance","CMS","Résistance CMS 0603  110 Ohm 5%"]
["Résistance","CMS","Résistance CMS 0603  121 Ohm 1%  SGN 22"]
["Résistance","CMS","Résistance CMS 0603  13 KOhm 5%  SGF 73"]
["Résistance","CMS","Résistance CMS 0603  130 Ohm 5% "]
["Résistance","CMS","Résistance CMS 0603  15 Ohm 5%  SGF 42"]
["Résistance","CMS","Résistance CMS 0603  18 KOhm 1%"]
["Résistance","CMS","Résistance CMS 0603  18 Ohm 5%  SGF 15"]
["Résistance","CMS","Résistance CMS 0603  180 Ohm 5%  SGF 41"]
["Résistance","CMS","Résistance CMS 0603  2.21 KOhm 1%  SGN 60"]
["Résistance","CMS","Résistance CMS 0603  2.26 KOhm 1%  SGN 32"]
["Résistance","CMS","Résistance CMS 0603  2.4 KOhm 1%  SGN 59"]
["Résistance","CMS","Résistance CMS 0603  2.49 KOhm 1%"]
["Résistance","CMS","Résistance CMS 0603  22 KOhm 5% 100mW RC01"]
["Résistance","CMS","Résistance CMS 0603  22.1 KOhm 1%  SGN 5"]
["Résistance","CMS","Résistance CMS 0603  221 KOhm 1%  SGN 21"]
["Résistance","CMS","Résistance CMS 0603  24 Ohm 5%  SGF 72"]
["Résistance","CMS","Résistance CMS 0603  24.9 Ohm 1%  SGN 28"]
["Résistance","CMS","Résistance CMS 0603  27 KOhm 5%  SGF 6"]
["Résistance","CMS","Résistance CMS 0603  270 KOhm 5%"]
["Résistance","CMS","Résistance CMS 0603  270 Ohm 5% "]
["Résistance","CMS","Résistance CMS 0603  300 Ohm 1%"]
["Résistance","CMS","Résistance CMS 0603  300 Ohm 5%"]
["Résistance","CMS","Résistance CMS 0603  301 Ohm 1%"]
["Résistance","CMS","Résistance CMS 0603  33 Ohm 5% 250mW  SGF 2"]
["Résistance","CMS","Résistance CMS 0603  330 Ohm 5%  SGF 17"]
["Résistance","CMS","Résistance CMS 0603  332 KOhm 1%"]
["Résistance","CMS","Résistance CMS 0603  332 Ohm 1%  SGN 8"]
["Résistance","CMS","Résistance CMS 0603  360 KOhm 5%  SGF 68"]
["Résistance","CMS","Résistance CMS 0603  39 KOhm  5%  SGF 24"]
["Résistance","CMS","Résistance CMS 0603  390 Ohm 1%"]
["Résistance","CMS","Résistance CMS 0603  4.7 MOhm 5% "]
["Résistance","CMS","Résistance CMS 0603  4.7 Ohm 5%  SGF 44"]
["Résistance","CMS","Résistance CMS 0603  430 Ohm 5%  SGF 65"]
["Résistance","CMS","Résistance CMS 0603  464 Ohm 1%  SGN 25"]
["Résistance","CMS","Résistance CMS 0603  475 KOhm 1%  SGN 3"]
["Résistance","CMS","Résistance CMS 0603  5.6 KOhm 5%  SGF 56"]
["Résistance","CMS","Résistance CMS 0603  51 Ohm 5%  SGF 53"]
["Résistance","CMS","Résistance CMS 0603  51.1 KOhm 1%  SGN 30"]
["Résistance","CMS","Résistance CMS 0603  56.2 KOhm 1%  SGN 31"]
["Résistance","CMS","Résistance CMS 0603  56.2 Ohm 1%"]
["Résistance","CMS","Résistance CMS 0603  590 Ohm 1%"]
["Résistance","CMS","Résistance CMS 0603  6.19 KOhm 1%  SGN 24"]
["Résistance","CMS","Résistance CMS 0603  6.8 KOhm 5%  SGF 29"]
["Résistance","CMS","Résistance CMS 0603  680 Ohm 5%  SGF 51"]
["Résistance","CMS","Résistance CMS 0603  75 KOhm 1%"]
["Résistance","CMS","Résistance CMS 0603  82 Ohm 5% "]
["Résistance","CMS","Résistance CMS 0805  0.51 Ohm 1% 125mW SR73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  0.51 Ohm 5% 125mW SR73K2A-TD J"]
["Résistance","CMS","Résistance CMS 0805  1 Ohm 5% 125mW"]
["Résistance","CMS","Résistance CMS 0805  1.05 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  1.05 KOhm 1% 125mW FCR05-F-T"]
["Résistance","CMS","Résistance CMS 0805  1.1 MOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  1.10 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  1.10 KOhm 1% 125mW MCR10 EZH F"]
["Résistance","CMS","Résistance CMS 0805  1.13 KOhm 1% 125mW"]
["Résistance","CMS","Résistance CMS 0805  1.13 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  1.2 KOhm 5% 125mW CR21-122-JL"]
["Résistance","CMS","Résistance CMS 0805  1.2 KOhm 5% 125mW FCR05JT-122"]
["Résistance","CMS","Résistance CMS 0805  1.21 KOhm 1% 125mW FCR05FT-1211"]
["Résistance","CMS","Résistance CMS 0805  1.24 KOhm 1% 125mW CR21-1241-FF"]
["Résistance","CMS","Résistance CMS 0805  1.24 KOhm 1% 125mW FCR05FT-1241"]
["Résistance","CMS","Résistance CMS 0805  1.33 KOhm 1% 125mW RC0805FR-071K33L"]
["Résistance","CMS","Résistance CMS 0805  1.47 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  1.5 KOhm 5% 125mW FCR05JT-152"]
["Résistance","CMS","Résistance CMS 0805  1.5 KOhm 5% 125mW MCR10 EZH J"]
["Résistance","CMS","Résistance CMS 0805  1.5 KOhm 5% 125mW RC0805"]
["Résistance","CMS","Résistance CMS 0805  1.54 KOhm 1% 125mW CRCW08051541FT"]
["Résistance","CMS","Résistance CMS 0805  1.6 KOhm 5% 125mW CR21-162-JF"]
["Résistance","CMS","Résistance CMS 0805  1.62 KOhm 1% 100mW RK73H2AFTD1K62"]
["Résistance","CMS","Résistance CMS 0805  1.62 KOhm 1% 125mW FCR05FT-1621"]
["Résistance","CMS","Résistance CMS 0805  10.2 KOhm 1% 125mW FCR05FT-1022"]
["Résistance","CMS","Résistance CMS 0805  10.5 KOhm 1% 125mW FCR05FT-1052"]
["Résistance","CMS","Résistance CMS 0805  10.5 Ohm 1% 125mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  107 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  107 Ohm 1% 125mW FCR05FT-1070"]
["Résistance","CMS","Résistance CMS 0805  11 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  11 Ohm 1% 125mW FCR05FT-11R0"]
["Résistance","CMS","Résistance CMS 0805  11.5 KOhm 1% 125mW FCR05FT-1152"]
["Résistance","CMS","Résistance CMS 0805  110 Ohm 1% 125mW FCR05FT-1100"]
["Résistance","CMS","Résistance CMS 0805  12 Ohm 1% 125mW RC0805FR-0712R"]
["Résistance","CMS","Résistance CMS 0805  12 Ohm 5% 100mW RK73K2A-TD J"]
["Résistance","CMS","Résistance CMS 0805  12.1 KOhm 1% 125mW RC12H"]
["Résistance","CMS","Résistance CMS 0805  12.4 KOhm 1% 125mW FCR05FT-1242"]
["Résistance","CMS","Résistance CMS 0805  12.7 KOhm 1% 125mW FCR05FT-1272"]
["Résistance","CMS","Résistance CMS 0805  120 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  121 Ohm 1% 125mW FCR05FT"]
["Résistance","CMS","Résistance CMS 0805  124 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  130 KOhm 1% 100mW MC01W08051130K"]
["Résistance","CMS","Résistance CMS 0805  130 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  130 Ohm 1% 125mW FCR05FT-1300"]
["Résistance","CMS","Résistance CMS 0805  133 KOhm 1% 125mW CR21-1333-FF"]
["Résistance","CMS","Résistance CMS 0805  133 KOhm 1% 125mW FCR05-F-T"]
["Résistance","CMS","Résistance CMS 0805  14 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  143 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  15 Ohm 5% 100mW RK73K2A-TD J"]
["Résistance","CMS","Résistance CMS 0805  150 KOhm 1% 125mW CR0805-FX-1503E"]
["Résistance","CMS","Résistance CMS 0805  150 KOhm 1% 125mW CR21-1503-FL"]
["Résistance","CMS","Résistance CMS 0805  150 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  150 Ohm 1% 125mW CR21-1500-FF"]
["Résistance","CMS","Résistance CMS 0805  150 Ohm 1% 125mW FCR05FT-1500"]
["Résistance","CMS","Résistance CMS 0805  16 KOhm 1% 125mW RC12H"]
["Résistance","CMS","Résistance CMS 0805  16 KOhm 1% 125mW V-D12-ZR0"]
["Résistance","CMS","Résistance CMS 0805  16.2 KOhm 1% 125mW FCR05-F-T"]
["Résistance","CMS","Résistance CMS 0805  16.5 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  16.9 KOhm 1% 125mW RC0805FR-0716K9"]
["Résistance","CMS","Résistance CMS 0805  18 Ohm 5% 100mW RK73K2A-TD J"]
["Résistance","CMS","Résistance CMS 0805  18.2 KOhm 1% 100mW MC"]
["Résistance","CMS","Résistance CMS 0805  18.2 KOhm 1% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  180 Ohm 1% 125mW CRCW08051800FT"]
["Résistance","CMS","Résistance CMS 0805  187 Ohm 1% 125mW CR21-1870-FF"]
["Résistance","CMS","Résistance CMS 0805  19.6 KOhm 0.1% RN73F2A-TD  SGH 2"]
["Résistance","CMS","Résistance CMS 0805  19.6 KOhm 1% 125mW CRCW08051962FT"]
["Résistance","CMS","Résistance CMS 0805  191 KOhm 1% 125mW FCR05FT-1913"]
["Résistance","CMS","Résistance CMS 0805  2.05 KOhm 1% 125mW CRCW08052051FT"]
["Résistance","CMS","Résistance CMS 0805  2.2 Ohm 5% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  2.21 KOhm 1% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  2.21 KOhm 1% 125mW FCR05-F-T"]
["Résistance","CMS","Résistance CMS 0805  2.21 Ohm 1% 125mW FCR05FT-2R21"]
["Résistance","CMS","Résistance CMS 0805  2.26 KOhm 1% CRCW08052261FT"]
["Résistance","CMS","Résistance CMS 0805  2.32 KOhm 1% 125mW CRCW08052K32FKEA"]
["Résistance","CMS","Résistance CMS 0805  2.32 KOhm 1% 125mW SCR05-2321-FP"]
["Résistance","CMS","Résistance CMS 0805  2.4 MOhm 1% 125mW CR21-2404-FF"]
["Résistance","CMS","Résistance CMS 0805  2.4 Ohm 5% 125mW CR0805-J-2R4-E"]
["Résistance","CMS","Résistance CMS 0805  2.67 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  2.74 KOhm 1% 125mW CR0805FX2741E"]
["Résistance","CMS","Résistance CMS 0805  20 Ohm 1% 125mW CR0805FX20R0E"]
["Résistance","CMS","Résistance CMS 0805  205 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  21 KOhm 1% 125mW CR21-2103-FF"]
["Résistance","CMS","Résistance CMS 0805  21.5 KOhm 1% 125mW FCR05FT-2152"]
["Résistance","CMS","Résistance CMS 0805  215 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  215 Ohm 1% 125mW FCR05FT-2150"]
["Résistance","CMS","Résistance CMS 0805  215 Ohm 1% 125mW RC0805FR-07215R"]
["Résistance","CMS","Résistance CMS 0805  22 Ohm 5% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  22.1 KOhm 1% 125mW FCR05FT-2212"]
["Résistance","CMS","Résistance CMS 0805  22.1 Ohm 1% 125mW FCR05FT-22R1"]
["Résistance","CMS","Résistance CMS 0805  22.6 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  22.6 KOhm 1% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  220 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  221 KOhm 1% 125mW CR21-2213-FF"]
["Résistance","CMS","Résistance CMS 0805  23.2 KOhm 1% 125mW FCR05FT-2322"]
["Résistance","CMS","Résistance CMS 0805  237 KOhm 1% 125mW FCR05FT-2373"]
["Résistance","CMS","Résistance CMS 0805  24 KOhm 1% 125mW CR21-2402-FF"]
["Résistance","CMS","Résistance CMS 0805  24.3 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  24.3 KOhm 1% 125mW FCR05FT-2432"]
["Résistance","CMS","Résistance CMS 0805  24.3 Ohm 1% 125mW FCR05FT-24R3"]
["Résistance","CMS","Résistance CMS 0805  24.9 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  24.9 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  24.9 KOhm 1% 125mW WCR0805-24K9F"]
["Résistance","CMS","Résistance CMS 0805  24.9 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  243 Ohm 1% 100mW RK73H2A-TD-F"]
["Résistance","CMS","Résistance CMS 0805  243 Ohm 1% 125mW FCR05FT-2430"]
["Résistance","CMS","Résistance CMS 0805  249 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  249 Ohm 1% 100mW RK73H2A-TD-F"]
["Résistance","CMS","Résistance CMS 0805  249 Ohm 1% 125mW CR21-2490-FF"]
["Résistance","CMS","Résistance CMS 0805  255 KOhm 1% 125mW FCR05FT-2553"]
["Résistance","CMS","Résistance CMS 0805  27 Ohm 1% 125mW RC0805FR-0727R"]
["Résistance","CMS","Résistance CMS 0805  27 Ohm 5% 100mW RK73K2A-TD J"]
["Résistance","CMS","Résistance CMS 0805  27 Ohm 5% 125mW FCR05JT-270"]
["Résistance","CMS","Résistance CMS 0805  27.4 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  27.4 KOhm 1% 125mW FCR05FT-2742"]
["Résistance","CMS","Résistance CMS 0805  27.4 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  270 KOhm 1% 100mW MC01W08051270K"]
["Résistance","CMS","Résistance CMS 0805  270 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  270 Ohm 1% 125mW CR21-2700-FF"]
["Résistance","CMS","Résistance CMS 0805  270 Ohm 1% 125mW MCR10 EZH J"]
["Résistance","CMS","Résistance CMS 0805  28 KOhm 1% 125mW CR21-2802-FF"]
["Résistance","CMS","Résistance CMS 0805  280 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  287 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  3.01 KOhm 1% 125mW RC0805FR-073K01"]
["Résistance","CMS","Résistance CMS 0805  3.16 KOhm 1% 125mW FCR05FT-3161"]
["Résistance","CMS","Résistance CMS 0805  3.3 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  3.3 Ohm 5% 125mW FCR05JT-3R3"]
["Résistance","CMS","Résistance CMS 0805  3.6 KOhm 1% 125mW CR21-3601-FF"]
["Résistance","CMS","Résistance CMS 0805  3.9 KOhm 1% 125mW RC0805FR-073K9"]
["Résistance","CMS","Résistance CMS 0805  3.92 KOhm 1% 125mW FCF05FT-3921"]
["Résistance","CMS","Résistance CMS 0805  30.1 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  300 Ohm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  300 Ohm 1% 125mW MCR10 EZH J"]
["Résistance","CMS","Résistance CMS 0805  301 KOhm 1% 125mW"]
["Résistance","CMS","Résistance CMS 0805  301 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  31.6 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  316 KOhm 1% 125mW RC0805FR-07316K"]
["Résistance","CMS","Résistance CMS 0805  32.4 KOhm 1% 125mW FCR05FT-3242"]
["Résistance","CMS","Résistance CMS 0805  33 Ohm 5% 125mW FCR05JT-330"]
["Résistance","CMS","Résistance CMS 0805  33.2 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  33.2 KOhm 1% 125mW FCR05FT-3322"]
["Résistance","CMS","Résistance CMS 0805  33.2 KOhm 1% 125mW RC12H"]
["Résistance","CMS","Résistance CMS 0805  330 KOhm 5% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  332 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  332 Ohm 1% 125mW FCR05FT-3320"]
["Résistance","CMS","Résistance CMS 0805  332 Ohm 1% 125mW RC0805FR-07332R"]
["Résistance","CMS","Résistance CMS 0805  34.8 KOhm 1% 125mW FCR05F-T-3482"]
["Résistance","CMS","Résistance CMS 0805  36.5 KOhm 1% 125mW FCR05FT-3652"]
["Résistance","CMS","Résistance CMS 0805  39 Ohm 5% 100mW RK73K2A-TD J"]
["Résistance","CMS","Résistance CMS 0805  39 Ohm 5% 125mW CR21-390-JF"]
["Résistance","CMS","Résistance CMS 0805  390 KOhm 1% 100mW MC01W08051390K"]
["Résistance","CMS","Résistance CMS 0805  390 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  390 KOhm 1% 125mW RC02H"]
["Résistance","CMS","Résistance CMS 0805  392 KOhm 1% 100mW RK73H2AFTD392K"]
["Résistance","CMS","Résistance CMS 0805  392 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  392 Ohm 1% 125mW WCR0805-392RF"]
["Résistance","CMS","Résistance CMS 0805  4.02 KOhm 1% 125mW FCR05-F-T"]
["Résistance","CMS","Résistance CMS 0805  4.22 KOhm 1% 125mW CR21-4221-FF"]
["Résistance","CMS","Résistance CMS 0805  4.22 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  4.32 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  4.42 KOhm 1% 125mW FCR05FT-4421"]
["Résistance","CMS","Résistance CMS 0805  4.64 KOhm 1% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  4.64 KOhm 1% 125mW FCR05FT-4641"]
["Résistance","CMS","Résistance CMS 0805  4.75 KOhm 0.1% RN73F2A-TD  SGH"]
["Résistance","CMS","Résistance CMS 0805  4.75 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  4.75 MOhm 1% 125mW CR21-4754-FF"]
["Résistance","CMS","Résistance CMS 0805  40.2 KOhm 1% 125mW FCR05FT-4022"]
["Résistance","CMS","Résistance CMS 0805  40.2 Ohm 1% 125mW FCR05-F-T"]
["Résistance","CMS","Résistance CMS 0805  44.2 KOhm 1% 100mW RK73H2A-TD -F"]
["Résistance","CMS","Résistance CMS 0805  44.2 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  464 Ohm 1% 125mW FCR05FT-4640"]
["Résistance","CMS","Résistance CMS 0805  47 Ohm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  475 KOhm 1% 100mW RMC"]
["Résistance","CMS","Résistance CMS 0805  475 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  48.7 KOhm 1% 125mW FCR05FT-4872"]
["Résistance","CMS","Résistance CMS 0805  487 Ohm 1% 100mW RK73H2A-TD-F"]
["Résistance","CMS","Résistance CMS 0805  487 Ohm 1% 125mW RC0805FR-07487R"]
["Résistance","CMS","Résistance CMS 0805  499 Ohm 1% 100mW RK73H2A-TD-F"]
["Résistance","CMS","Résistance CMS 0805  499 Ohm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  5.11 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  5.11 KOhm 1% 125mW FCR05FT-5111"]
["Résistance","CMS","Résistance CMS 0805  51.1 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  51.1 Ohm 1% 125mW CR21-51R1-FF"]
["Résistance","CMS","Résistance CMS 0805  510 Ohm 1% 125mW CR21-5100-FF"]
["Résistance","CMS","Résistance CMS 0805  511 KOhm 1% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  511 KOhm 1% 125mW CR21-5113-FF"]
["Résistance","CMS","Résistance CMS 0805  511 Ohm 1% 100mW RK73H2A-TD-F"]
["Résistance","CMS","Résistance CMS 0805  511 Ohm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  549 Ohm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  549 Ohm 1% 125mW RC0805FR-07549R"]
["Résistance","CMS","Résistance CMS 0805  56 Ohm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  56.2 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  56.2 KOhm 1% 125mW CR21-5622-FF"]
["Résistance","CMS","Résistance CMS 0805  562 KOhm 1% 100mW RMC"]
["Résistance","CMS","Résistance CMS 0805  6.34 KOhm 0.1% RN73F2A-TD  SGH 1"]
["Résistance","CMS","Résistance CMS 0805  6.34 KOhm 1% 125mW FCR05FT-6341"]
["Résistance","CMS","Résistance CMS 0805  6.49 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  6.49 KOhm 1% 125mW FCR05FT-6491"]
["Résistance","CMS","Résistance CMS 0805  6.8 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  6.8 Ohm 5% 125mW CR0805"]
["Résistance","CMS","Résistance CMS 0805  6.81 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  60.4 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  619 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  64.9 KOhm 1% 125mW FCR05-F-T"]
["Résistance","CMS","Résistance CMS 0805  66.5 KOhm 1% 125mW CR21-6652-FF"]
["Résistance","CMS","Résistance CMS 0805  68.1 KOhm 1% 125mW RC0805-FR-0768K1"]
["Résistance","CMS","Résistance CMS 0805  68.1 Ohm 1% 125mW FCR05FT-68R1"]
["Résistance","CMS","Résistance CMS 0805  68.1 Ohm 1% 125mW WCR0805-68R1FI"]
["Résistance","CMS","Résistance CMS 0805  680 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  681 KOhm 1% 125mW FCR05FT-6813"]
["Résistance","CMS","Résistance CMS 0805  71.5 KOhm 1% 125mW FCR05FT-7152"]
["Résistance","CMS","Résistance CMS 0805  71.5 KOhm 1% 125mW RC0805FR-0771K5"]
["Résistance","CMS","Résistance CMS 0805  71.5 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  750 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  78.7 KOhm 1% 125mW RC0805FR-0778K7"]
["Résistance","CMS","Résistance CMS 0805  78.7 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  8.2 KOhm 1% 125mW CR21-8201-FF"]
["Résistance","CMS","Résistance CMS 0805  8.2 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  8.2 Ohm 1% 125mW RC0805FR-078R2"]
["Résistance","CMS","Résistance CMS 0805  8.25 KOhm 1% 125mW FCR05FT-8251"]
["Résistance","CMS","Résistance CMS 0805  8.25 Ohm 1% 125mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  82.5 KOhm 1% 125mW ERJ6ENF8252V"]
["Résistance","CMS","Résistance CMS 0805  820 Ohm 1% 125mW FCR05FT-8200"]
["Résistance","CMS","Résistance CMS 0805  825 Ohm 1% 125mW WCR0805-825RF"]
["Résistance","CMS","Résistance CMS 0805  866 Ohm 1% 100mW RK73H2A F TD"]
["Résistance","CMS","Résistance CMS 0805  9.09 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  9.31 KOhm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  9.53 KOhm 1% 125mW CR21-9531-FF"]
["Résistance","CMS","Résistance CMS 0805  9.76 KOhm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 0805  90.9 KOhm 1% 125mW FCR05FT-9092"]
["Résistance","CMS","Résistance CMS 0805  90.9 Ohm 1% 100mW RK73H2A-TD F"]
["Résistance","CMS","Résistance CMS 0805  90.9 Ohm 1% 125mW CR21-90R9-FF"]
["Résistance","CMS","Résistance CMS 0805  95.3 KOhm 1% 125mW CRCW0805"]
["Résistance","CMS","Résistance CMS 0805  976 Ohm 1% 125mW CRCW0805 BC"]
["Résistance","CMS","Résistance CMS 1206  1 KOhm 0.1%  SGL 1"]
["Résistance","CMS","Résistance CMS 1206  10 KOhm 0.1%  SGL 2"]
["Résistance","CMS","Résistance CMS 1206  249 KOhm 0.1% 400mW PTN1206E2493B"]
["Résistance","CMS","Résistance CMS 1218  1.2 KOhm  5% 1W  SGP 1"]
["Résistance","CMS","Résistance CMS 2010  0.05 Ohm 1%  SGG 1"]
["Résistance","CMS","Résistance CMS 2010  1.5 KOhm 5% (RM73B2HTE152J)  SGG 2"]
["Résistance","CMS","Résistance CMS 2512  0.82 Ohm 5% 1W FCR25JP-R820"]
["Résistance","CMS","Résistance CMS 2512  1.5 Ohm 1% 1W RMC1-1R5JTE"]
["Résistance","CMS","Résistance CMS 2512  150 Ohm 5% 1W FCR25JP-151"]
["Résistance","CMS","Résistance CMS 2512  270 Ohm 5% 250mW RK73K3A-TE"]
["Résistance","CMS","Résistance CMS 2512  47 Ohm 5% 1W CR63-470-JQ"]
["Résistance","CMS","Résistance CMS 2512  6.8 Ohm 5% 1W FCR25-J-P"]
["Résistance","CMS","Résistance CMS 2512  8.2 Ohm 5% 1W FCR25JP-8R2"]
["Résistance","De puissance","Résistance de puissance 1.2 KOhm 5% 1W  PGP 61"]
["Résistance","De puissance","Résistance de puissance 10 KOhm 1/8W"]
["Résistance","Métal","Résistance métal TRAD 1.2 KOhm 5% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 1.5 KOhm 5% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 10 KOhm 5% 1/8W  PGD 4"]
["Résistance","Métal","Résistance métal TRAD 10 MOhm 5% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 10 Ohm 1% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 100 KOhm 5% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 22 KOhm 1% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 3.3 KOhm 5% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 30.1 KOhm 1% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 330 Ohm 5% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 4.12 KOhm 1% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 43.2 KOhm 1% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 6.8 Ohm 1% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 68 KOhm 5% 1/4W"]
["Résistance","Métal","Résistance métal TRAD 820 KOhm 1/4W 5% MET"]
["Résistance","Miniself","Résistance Minimelf SMM0204  1 KOhm 1%   SGJ 4"]
["Résistance","Miniself","Résistance Minimelf SMM0204  1 MOhm 1%   SGJ 5"]
["Résistance","Miniself","Résistance Minimelf SMM0204  9.09 Ohm 1%   SGJ 2"]
["Self",null,"Self CMS 1210 NL322522T-1R0J 1µH 5% 7.96MHz 400mA  PNS 103"]
["Self",null,"Self CMS 1210 NL322522T-1R5J 1.5µH 5% 7.96MHz 370mA  PNS 118  "]
["Self",null,"Self CMS CD54-220MC  22μH 20%  PNS 141"]
["Self",null,"Self CMS NFM4516R13C102RT1  EMI Filter 0.3A 100VDC SMD  PNS 178  "]
["Support teflon",null,"Support Teflon Quartz  PXD 12"]
["Transistor","CMS","Transistor CMS BC 847B LT1 NPN  SOT23"]
["Transistor","CMS","Transistor CMS BCX 71 G E-6327 PNP SOT23  SJS 142"]
["Transistor","CMS","Transistor CMS BFR 31 LT1 JFET N-CH 25V SOT23  SJS 144  "]
["Transistor","CMS","Transistor CMS BFT 25A  2GHz NPN SOT23  SJS 58"]
["Transistor","CMS","Transistor CMS BSR 13 NPN 30V SOT23  SJS 100  "]
["Transistor","CMS","Transistor CMS BSR 15 PNP 40V SOT23  SJS 67  "]
["Transistor","CMS","Transistor CMS BSR 17A NPN 40V SOT23  SJS 113  "]
["Transistor","CMS","Transistor CMS BSS 123 LT1 Mosfet faible 100V 170mA Canal N SOT23  SJS 127  "]
["Transistor","CMS","Transistor CMS BSS 123 LT1G Canal N SOT23"]
["Transistor","CMS","Transistor CMS FMMT 720 TA Signal bipolaire faible PNP SOT23  SJS 60  "]
["Transistor","CMS","Transistor CMS NDS352 AP MOSFET Canal P 30V SOT23   SJS 184  "]
["Transistor","CMS","Transistor CMS PDTC 114ET NPN SOT23  SJS 228"]
["Transistor","CMS","Transistor CMS PMBT 2907A  600mA 60V PNP SOT23   SJS 17"]
["Transistor","CMS","Transistor CMS PMBT 3640 PNP 1 GHz switching SOT23  SJS 40  "]
["Transistor","CMS","Transistor CMS PMBT 3906 PNP 200mA 40V SOT23  SJS 63"]
["Transistor","CMS","Transistor CMS ZVP 3306 FTA Canal P 60V SOT23  SJS 104  "]
["Transistor","TRAD","Transistor TRAD BF 423 TO92  PJT 17"]
["Transistor","TRAD","Transistor TRAD BS 170 TO92  PJT 6"]
["Transistor","TRAD","Transistor TRAD TL 431CLP TO92  PJT 47"]